2021 Orthoimagery – Region of Peel
Orthoimagery (aerial photography) covering all of Peel Region. The imagery is provided at a spatial resolution of 7.5 centimetres.
Orthoimagery is foundational to mapping work. It's used to create data, perform analysis, mapping, management of resources, planning, and as background data in maps.
[bookmark: _Hlk113977746]Available products
Orthorectified mosaics - full resolution images (7.5cm) in GeoTIFF format using lossy (JPEG YCbCr @ 75%) compression:
· Peel Region +1km buffer - 39 Gigabytes (self-service download GeoTIFF)
· Download the statistics file for the GeoTIFF.
Orthorectified mosaics – full resolution images (7.5cm) in lossless MrSID format:
· Brampton +1km buffer - 22 Gigabytes
· Caledon +1km buffer - 40.7 Gigabytes
· Mississauga +1km buffer - 21 Gigabytes
· Peel Region +1km buffer - 82 Gigabytes
Specifications
· Spatial resolution - 7.5cm
· Acquisition dates: March 19, 25, 30; April 2, 3, 4 2021
· Image format: Lossless MrSID
· Bands: 3-band rendered RGB
· Canopy coverage: leaf-off
· Projection: NAD 1983 UTM Zone 17N (EPSG: 26917)
· Horizontal/vertical accuracy: ±20cm
· Collection contractor: First Base Solutions Inc.
Accessing the data
Due to the large size of the dataset, access is provided upon request.  Only the lossy GeoTIFF is available for self-serve download (see links above).  The only method of access will be by download.
To receive a download link, please contact peeldatacentre@peelregion.ca.  In your email, make sure you tell us that you're looking for orthoimagery and what year you're looking to download.
License
The 2021 orthoimagery is released under the Open Data Licence for The Regional Municipality of Peel (Version 1.0).

