2020 Orthoimagery – Region of Peel
Orthoimagery (aerial photography) covering all of Peel Region. The imagery is provided at a spatial resolution of 15 centimetres.
Orthoimagery is foundational to mapping work. It's used to create data, perform analysis, mapping, management of resources, planning, and as background data in maps.
[bookmark: _Hlk113977746]Available products
Orthorectified mosaics – full resolution images (15cm) in lossless MrSID format:
· Brampton +1km buffer – 2.8 Gigabytes
· Caledon +1km buffer – 5.7 Gigabytes
· Mississauga +1km buffer – 3.2 Gigabytes
· Peel Region +1km buffer – 10.4 Gigabytes (self-serve download link)
Specifications
· Spatial resolution - 15cm
· Acquisition dates: April 6 (Mississauga); May 22, 31; June 1 2020
· Image format: Lossless MrSID
· Bands: 3-band rendered RGB
· Canopy coverage: leaf-off (Mississauga), leaf-on (Brampton and Caledon)
· Projection: NAD 1983 UTM Zone 17N (EPSG: 26917)
· Horizontal/vertical accuracy: ±20cm
· Collection contractor: First Base Solution Inc.
Accessing the data
Due to the large size of the dataset, access is provided upon request.  However, the Region of Peel mosaic is available as a self-serve download using the link above.  The only method of access will be by download.

To receive a download link, please contact peeldatacentre@peelregion.ca.  In your email, make sure you tell us that you're looking for orthoimagery and what year you're looking to download.
License
The 2020 orthoimagery is released under the Open Data Licence for The Regional Municipality of Peel (Version 1.0).
